EXAM 2 – DSIT 100

1. Building Area is defined as::
a. Area inside surrounding exterior walls  b. Area within surrounding exterior walls  c. Area excluding surrounding exterior walls  d. Area of all floors
2. Allowable building height, area and number of stories is based on:
a. Sprinkler system
b. Occupancy type
c. Fire resistance
d. Occupancy type and type of construction
3. Accessory occupancies:
a. Can be located on one level only  


b. Occupy less than 10% of primary occupancy 

c.     Occupy less than 10% of total building area  

d. Have to be less than 50 occupants total
4. Subcategory division of F Occupancy is based on:
a. Moderate or low hazard
b. Quantity of occupants
c. Low or high hazard
d. Value of products
5. Mixed Occupancies …:
a. … are always required to be separated.



b. … can be separated or non-separated

c.     … are allowed when all but one are accessory to the main occupancy 
d. … not allowed in combustible construction
6. What is the name of current California Green Building Code:
a. GreenBuild
b. 2009 LEED
c. 2010 California Green Building Code
d. 2010 CalGreen
7. Adding fire alert and sprinkler system can:
a. Increase allowable building height  b. Increase building allowable height and area  c. Increase fire rating  d. Increase number of occupants
8. Which of these do NOT enforce the Building Code?
a. Building Official
b. Contractor
c. Designer
d. Client
9. Which of these types of building use would qualify for E occupancy:
a. College campus
b. Church

c. Elementary school
d. Employee training center
10. What are the main goals for the Building Code:
a. Security
b. Life Safety and Property Protection
c. Life Preservation
d. Structural Integrity of Buildings
11. Full name of current California Building Code is:
a. 2009 International Building Code
b. 2010 CCR Title 24 Part 2
c.2011 California Building Code – Part 2
d. 2009 Title 24 Building Code

12. Which issuance of Americans with Disabilities Act is current California Building Code enforcing:

a. 2009

b. 2010
c. 2004
d. 1991
13. Non-Combustible material:
a. … will not ignite or burn 
b.  … will not burn

c. … is fire resistant 
d. … has passive fire resistance
14. Passive fire resistance is based on:
a. Fire rating of materials
b. Sprinkler system  
 c. Construction of materials and assemblies 
d. ASTM standard
15. In which order would you consult the Chapters of the California Building Code on a TYPICAL project:

a. Chapters 3, 4, 5, 6

b. Chapters 4, 5, 6, 7

c. Chapters 3, 5, 10, 11
d. Chapters 3, 5, 6, 10
16. Difference between Type I and Type II occupancy is in:
a. Non-combustible vs. combustible interior construction

b. Passive vs. active fire resistance

c.     Fire sprinklers





d. Non-combustible vs. combustible exterior construction
17. Which one of these is a characteristic of ALL I Occupancies:
a. Non-ambulatory occupants
b. Restraint
c. Supervised environment
d. More than 50 occupants
18. Building occupancy is classification of use based on:
a. Fire resistance and number of occupants   b. Fire safety and relative hazard involved   c. Capability for preservation   d. Building function
19. Separated occupancies are required …:
a. … to have fire rated separation per Table 508.3.3


b. … to be separated based on the building height

c.     … to have rated or non-rated separation based on Table 508.3.3
d. … to be located in different buildings
20. Type III Construction type uses non-combustible materials for the exterior and combustible materials for:
a. Residential applications
b. Occupancy Separation
c. Roof Construction
d. Interior Construction
